# ID 50473

Switch on the backward motion memory without memory impossible.
Description | Sufficient memory capacity must be available to activate the backward motion memory for backward motion. P-STUP-00033. For more information on backward motion, see [FCT-C7// Section: Forward/backward motion on the path]
Response | Class | 1 | None.
Solution | Class | 1 | Release memory for backward motion P-STUP-00033.
Error type | -