# Settings for measurement

This section summarises the axis-specific parameters for measurement.

## Notice

The measurement parameters are used for a specific application. The measurement functions are described in [PROG] in greater detail.

## Additional information

- Define axis as measurement axis (P-AXIS-00118)
- Probe stroke for measurement types 2 and 4 (P-AXIS-00086)
- Measurement speed for measurement type 2 (P-AXIS-00215)
- Measurement travel offset for measurement type 2 (P-AXIS-00114)
- Measurement travel offset for all measurement types (P-AXIS-00467)
- New measurement signal parameters (kenngr.measure.*)
- Measurement parameters for SERCOS drives
- Parameters for measuring travel on fixed stop
- Abortion of measuring order at reset (P-AXIS-00378)
- Actuation time delay of probe (P-AXIS-00487)
- Old probing signal parameters (up to CNC Build V2.11.2019.14)