# ID 60290

Tool change with changing gear ratio only permitted in standstill.
Description | If a tool with a gear stage is changed in or out, a gear switching takes place in the position controller. Therefore, changing a tool with a gear ratio is only permitted in standstill due to security reasons.
Response | Class | 6 | Axis stop and abortion of NC-program.
Solution | Class | 6 | Stop the spindle before changing the tool.
Parameter | %1: |
Logical axis number @@P-AXIS-00016 of the concerned spindle
%2: | Current value [-]
Numerator P-TOOL-00016 of tool gearbox ratio
%3: | Current value [-]
Denominator P-TOOL-00017 of tool gearbox ratio
%4: | Current value [-]
Reversal of rotation direction P-TOOL-00018 by tool
%5: | Current value [-]
Error type | 1, Error message from NC program.