# Separate preselection and activation

With multi-step transformations, kinematic IDs are preselected by an extended #KIN ID command:

Syntax:
#KIN ID [ <kin_id_first_step> , <kin_id_second_step> ]

<kin_id_first_step> | Set the kinematic ID number of the first transformation step
<kin_id_second_step> | Set the kinematic ID number of the second transformation step

The following keywords can also be used instead of kinematic IDs:

NONE | Deselect the kinematic ID
DEFAULT | Set the default kinematic ID from the channel list

## Notice

Select(deselect the transformation by using the default command #TRAFO ON/OFF.

## Example

Nxx #KIN ID [86,1] ;Preselect kinematic 86 and 1

Nxx #KIN ID [86,NONE] ;Preselect kinematic 86 and deselect 1

;..or address only first step to always deselect second step

Nxx #KIN ID [86] ;Preselect kinematic 86 and deselect 1

Nxx #KIN ID [NONE,3] ;Deselect kinematic 86 and select 3

Nxx #KIN ID [NONE,NONE] ;Deselect both kinematics

;..or address only first step to always deselect second step

Nxx #KIN ID [NONE] ;Deselect both kinematics

Nxx #KIN ID [DEFAULT,1] ;Preselect default kinematic and 1

Nxx #KIN ID [DEFAULT, DEFAULT] ;Preselect default kinematics for

;both steps

Nxx #KIN ID ;Preselect default kinematics for

;both steps

:

Nxx #TRAFO ON ;Activate kinematic transformation as per preselection

;causes errors if both kinematics are NONE

:

Nxx #TRAFO OFF ;Deactivate kinematic transformations