# ID 110294

Changing the D/A-hardware id requires a restart.
Description | The parameter P-AXIS-00049 that indicates the system-wide unique hardware identification for the D/A area, cannot be changed while CNC kernel is running. The new hardware identification is not transferred, the previous active hardware identification remains valid.
Response | Class | 1 | None.
Solution | Class | 1 | Change the entry P-AXIS-00049 only in configuration mode or when CNC is disabled.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis.
%2: | Current value [-]
Current value of P-AXIS-00049.
%3: | Corrected value [-]
Corrected value of P-AXIS-00049.
Error type | 2, Error message by data transfer from parameter list into control device.