# Maximum number of logged events (P-STUP-00091)

P-STUP-00091 | Maximum number of entries in the history buffer
Description | The CNC offers the options of filing events in a history memory (logging entries). This parameter defines the maximum number of logged events. If there are more entries, the oldest one is overwritten.
Parameter | configuration.axes_manager.log_entry_number
Data type | UNS32
Data range | 0 ... MAX(UNS32)
Dimension | ----
Default value | 0
Remarks |