# Requesting of a SAI axis at RESET (P-AXIS-00251)

P-AXIS-00251 | Requesting of a SAI axis at RESET
Description | An SAI (or spindle) can be commanded via #PUTAX by a channel to release its axis. If the SAI receives a RESET from the same channel and it has no axis under control, this SAI requests the axis again automatically.
Parameter | kenngr.auto_call_ax
Data type | BOOLEAN
Data range | 0/1
Axis types | T, R, S
Dimension | T: ---- | R,S: ----
Default value | 0
Drive types | ----
Remarks |