# Behaviour at STOP marks during backward movement (P-CHAN-00308)

P-CHAN-00308 | Response at STOP marks during backward movement
Description | Suppress stop at STOP during backward movement.
Parameter | forward_backward.disable_stop_backward
Data type | BOOLEAN
Data range | 0: The movement stops at the STOP mark during backward movement. 1: The STOP mark is ignored during backward movement
Dimension | ----
Default value | 0
Remarks | This parameter is available as of CNC Build V3.1.3039.01.