# ID 110311

Reduced maximum velocity P-AXIS-00214 is greater than the maximum axis velocity.
Description | The reduced maximum velocity for G01 P-AXIS-00214 was specified greater than the maximum axis velocity.
Response | Class | 1 | The velocity is assigned the maximum axis velocity.
Solution | Class | 1 | Correct the value in the parameter list.
Parameter | %1: | Logical axis number [-]
P-AXIS-00016
%2: | Current value [1µm/s or 0.001°/s]
P-AXIS-00214
%3: | Limit value [1µm/s or 0.001°/s]
P-AXIS-00212
%4: | Corrected value [1µm/s or 0.001°/s]
P-AXIS-00214
Error type | 2, Error message on data transfer of parameter lists to controller.