# ID 13125

Number of infeeds for thread cutting (@P__) is incorrect, must be a positive integer.
Description | Error in the definition of parameter @P__ for the thread type. @P__ must be a positive integer.
Response | Class | - | Error: Transition to error state. Complete reset of the NC channel necessary.
Solution | Class | - | Check and correct the definition of infeed motions (@P__).
Parameter | %1: | Error value
Affected input parameter @P__.
Error type | 1, Error message from the NC program