# ID 20746

SPLINE parameter is out of data format.
Description | When programming the commands #AKIMA TRANS [..] / #AKIMA STARTVECTOR/ #AKIMA ENDVECTOR or #SET ASPLINE MODE [...] or #SET ASPLINE STARTTANG/ZIELTANG, there is a spline parameter outside of the permissible data range.
Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify the spline parameter.
Parameter | %1: | Error value [-]
%2: | Lower limit value [-]
%3: | Upper limit value [-]
Error type | Abort NC program processing.