# ID 13327

Invalid matrix initialization.
Description | When a matrix was created, an invalid initialization variant was defined. See the documentation for a list of all available variants.
Response | Class | - | Error: Transition to error state. Complete reset of the NC channel necessary.
Solution | Class | - | Check parameter setting and correct input parameters for the matrices in the calling NC program/cycle.
Parameter | %1: | Identification number
Index of incorrect parameter
%2: | Current value
Invalid initialization identifier
Error type | 1, Error message from NC program.