# Integers <int>

Integers are specified without a decimal point. The internally permissible value range corresponds to "long integer” variables in the C programming language, i.e. the range from -2.14*109 to +2.14*109.

If internal calculation uses the unit 0.1 µm, the numerical range when values are entered in mm is between –2.14*105and +2.14*105. This corresponds to a motion path of over 400 metres. Due to an internal limitation in the position controller, the motion path is limited to half, i.e. to just over 200 metres.

Where negative numerals are preceded by "-", positive numerals do not require the prefix "+".