# ID 20801

Remaining path for edge bending is out of data format or out of permissible value range.
Description | The programmed residual path at edge bending that can be entered via the variable V.G.RW in the NC program, or which can be defined via the channel parameter P-CHAN-00030 exceeds the permissible numerical range.
Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify the channel parameter P-CHAN-00030 or the programmed variable V.G.RW in the NC program.
Parameter | %1: | Error value [-]
%2: | Lower limit value [-]
%3: | Upper limit value [-]
Error type | 1, Error message from NC program.