# ID 110244

Logical axis number of master axis is missing for GANTRY operation.
Description | The axis is marked as slave axis of a gantry link in P-AXIS-00015 parameter, but there is a missing entry for leading master axis P-AXIS-00070.
Response | Class | 3 | None.
Solution | Class | 7 | Use correct entry for logical axis number P-AXIS-00070 of leading master axis of the gantry link.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis.
%2: | Logical axis number [-]
Current logical axis number of the master axis P-AXIS-00070.
Error type | 2, Error message by data transfer from parameter list into control device.