# ID 40067

FB error: MCV_RedSpeedZone. Value at input "ZoneNr" is invalid.
Description | Zones can be defined for an axis in the respective parameter list (P-AXIS-00085, P-AXIS-00097) in which the motion is carried out at reduced speed after a corresponding job. The job specifies which of the zones configured in the parameter list (1 or 2) is to be activated.

The error message is displayed if the value at the input "ZoneNr" points to an undefined zone.

Response | Class | - | There is no interaction with the Motion Controller.
Solution | Class | - | Correct value at input "ZoneNr" so that value points to a defined zone.
Error type | -