# ID 13123

Thread size not defined.
Description | If a thread tapping drill with countersink (special tool (P[6], see Section: Cyclic-specific tool data) is used for machining, the metric thread size is needed to calculate countersink motion. This message is generated if the thread size is not assigned by default in the tool parameters. (P[7] see Section: Cyclic-specific tool data).
Response | Class | - | Error: Transition to error state. Complete reset of the NC channel necessary.
Solution | Class | - | Check and define thread size and correct tool parameters P[7].
Error type | 1, Error message from the NC program