# ID 120498

No workspace monitoring possible with activated coordinate system.
Description | When a machine coordinate system (#CS ON) is active, workspace monitoring cannot take place given the current development status. This function will be developed in the future. For the present status, ask your controller supplier.
Response | Class | 6 | Movement stop.
Solution | Class | 6 | Disable the CS function
Error type | 1, Error message from NC program.