# ID 120579

Plane change in work or protection area definition not permitted.
Description | The machining plane may not be changed during the definition of a work or protection area (see [FCT-C14// Definition of work and protection areas]). Example with error: #CONTROL AREA START [ID1 PROT CIRC MIN_EXCUR=-50 MAX_EXCUR=50] G01 Y100 Z100 F1000

G19

G02 G162 Y100 Z100 J-100 F1000

#CONTROL AREA END

Corrected example:

G19

#CONTROL AREA START [ID1 PROT CIRC MIN_EXCUR=-50 MAX_EXCUR=50]

G01 Y100 Z100 F1000

G02 G162 Y100 Z100 J-100 F1000

#CONTROL AREA END

Response | Class | 2 | Abort NC program processing.
Solution | Class | 6 | Check and modify the NC program
Parameter | %1: | Identification number [-]
Identifier of affected work or protection area
Error type | 1, Error message from NC program.