# ID 20569

In NC block #COMMENT END has to be programmed exclusively.
Description | After the #COMMENT END command, no further NC commands are permitted in the same NC block. Example: Wrong: N10 #COMMENT BEGIN :

N30 #COMMENT END X100 F1000 G01 F100

:

N1000 M30

Correct:

N10 #COMMENT BEGIN

:

N30 #COMMENT END

N40 X100 F1000 G01 F100

:

N1000 M30

For further information see [PROG// Section: Cross-block comments

Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and adjust NC program sequence. Move the not permissible NC-commands to the following NC-block. Note: Only with #ACHSE, #PSET and #PRESET further NC commands are permitted in the same NC block.
Error type | 1, Error message from NC program.