# ID 110465

Denominator for torque scaling must not be zero.
Description | The denominator of the torque scaling factor (see P-AXIS-00326) was assigned the value 0.
Response | Class | 1 | Warning output, torque scaling factor is set internally to zero.
Solution | Class | 1 | P-AXIS-00326 must have a value other than 0 assigned.
Parameter | %1: | Logical axis number [-]
Logical axis number (see P-AXIS-00016).
%2: | Error value [-]
Incorrect value of P-AXIS-00326.
%3: | Corrected value [-]
Corrected value of P-AXIS-00326.
%4: | Corrected value [-]
Incorrect value of P-AXIS-00325.
Error type | 2, Error message by data transfer from parameter list into control device.