# ID 50169

During block search not allowed interpolator control data received.
Description | With active block search mode, some functions or functionalities, such as manual operation mode or homing, are not supported. For further information see FCT-C6.
Response | Class | 1 | None.
Solution | Class | 1 | Remove activation of function on reported block number of NC program.
Error type | 1, Error message from NC program.