# ID 13211

Measuring velocity @P10 is not defined or wrong.
Description | The defined measuring velocity must be greater than zero. It is either not defined or incorrectly defined.
Response | Class | - | Error: Transition to error state. Complete reset of the NC channel necessary.
Solution | Class | - | Check parameter setting and correct input parameters.
Error type | 1, Error message from the NC program