# ID 51082

Non-homed axis is to be moved although prog_move_req_homing is set.
Description | A non-homed axis is to be interpolated although the parameter P-AXIS-00277 (kenngr.prog_move_requires_homing) is set for this axis.
Response | Class | 6 | Abrupt stop for all axes.
Solution | Class | 6 | Conduct a rest; home the axis before interpolating it. Or do not set P-AXIS-00277.
Parameter | %1: | Logical axis number
Logical axis number Axis parameters of the axis affected
Error type | -