# ID 110398

cam_gear: Number of values not allowed for means of value calculation.
Description | The number of values P-AXIS-00301to be used for averaging in master actual value filtering is not permitted.
Response | Class | 1 | Warning output. The value for P-AXIS-00301 is corrected automatically.
Solution | Class | 1 | Adjust the value for P-AXIS-00301 accordingly.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis.
%2: | Current value [-]
Current value of P-AXIS-00301.
%3: | Corrected value [-]
Corrected value of P-AXIS-00301.
Error type | 2, Error message by data transfer from parameter list into control device.