# ID 120268

Change of spline type while spline interpolation is active.
Description | While active Akima or B-spline interpolation, spline type cannot be changed. For more information on spline function, see [PROG// Section: Akima spline interpolation]. [PROG// Section: B spline interpolation].
Response | Class | 2 | Program execution stop.
Solution | Class | 6 | Before change of spline type in CNC program deactivation of spline function is necessary.
Error type | 1, Error message from NC program.