# ID 20048

Centre point coordinate within linear motion block ignored.
Description | The centre point coordinate (I,J,K) of the linear block (G01) is ignored. Example: Wrong: N10 G00 X0 Y0 Z0 N20 G01 I10 X10 F1000

N1000 M30

Correct:

N10 G00 X0 Y0 Z0

N20 G01 X10 F1000

`N1000 M30`

Response | Class | 1 | Continue NC program processing.
Solution | Class | 1 | Check and modify NC program. Remove the Centre point co-ordinates (I,J,K).
Error type | 1, Error message from NC program.