# Slave positions outside the modulo range

If the gear ratio between the master and slave is to be very large, it may be necessary to define slave positions that lie outside the modulo range.

This is why slave positions outside the modulo range are not transformed into it, but are used without change as an interpolation point.

The following figure shows such a table and the profile thus run through.

## Programing Example

Table with large transformation, endless negative

Tablename = extremetable4 # Table name

Table-ID = 414 # Table-ID

Tabletype = 7 # Table type

Function type = 5 # Interpolation type

Lines = 8 # Number of lines

Begintable # Beginning of table

0 0

200000 0

900000 -500000

1800000 -10000000

2100000 -16000000

2700000 -12000000

3200000 -19000000

3400000 -20000000

EndTable

Table with large transformation, endless negative