# ID 90109

Number of non-relevant buffered blocks was exceeded.
Description | The number of non-relevant blocks, which are buffered with perpendicular selection and deselection, was exceeded. Non-relevant blocks contain no motion data for TRC blocks, e.g. technology functions.
Response | Class | 2 | Abort NC program processing.
Solution | Class | 6 | Modify the NC program: Interrupt sequence of non-relevant blocks by a relevant block.
Error type | 1, Error message from NC program.