# ID 20804

Temporary transition into machine coordinate system is inactive.
Description | Deselection of the temporary transition to machine coordinate system with the command #MCS OFF has no effect because the temporary transition is not active.
Response | Class | 1 | Continue NC program processing.
Solution | Class | 1 | Remove the #MCS OFF command.
Error type | 1, Error message from NC program.