# ID 20205

Double-programmed centre point coordinate.
Description | In the same NC block, a centre point coordinate was programmed several times. Example: Wrong: N10 G00 X0 Y0 Z0 N20 G02 I10 I20 J30 F2000

:

`N1000 M30`

Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify NC program. Remove the redundant centre point coordinate.
Error type | 1, Error message from NC program.