# ID 120095

Deselection only possible with active spline interpolation.
Description | Spline interpolation can only be deselected after this function was selected. For more information on spline interpolation, see [PROG// Section: Akima spline interpolation].
Response | Class | 2 | Program abort.
Solution | Class | 6 | Check CNC program, select spline function with G151 .
Parameter | %1: | Current value [-]
Error type | 1, Error message from NC program.