# ID 70320

Activation of plane compensation not possible since compensation value list is invalid.
Description | Could not activate plane compensation since no compensation value list exists or it contains errors. See also: [FCT-C5// Section: Plane compensation] [COMP// Section: Plane compensation]
Response | Class | 7 | Stop axis, plane compensation remains inactive
Solution | Class | 6 | Correct Compensation value list see [COMP]
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of axis affected
Error type | 11, Error message from position controller.