# Smoothing factor (P-CHAN-00827)

P-CHAN-00827 | Smoothing factor
Description | The parameter specifies the weighting of the current measured value. Example: With a smoothing factor of 0.5, the current value is applied to the average value at a rate of 50%.
Parameter | dist_ctrl[i].smoothing_factor (where i=0)
Data type | REAL64
Data range | 0 < P-CHAN-00827 ≤ 1.0
Dimension | [-]
Default value | 0.7
Remarks | Available as of Build V3.1.3080.12 or V3.1.3107.44