# ID 110560

Position window for rapid traverse cannot be used with spindles.
Description | For a spindle (see P-AXIS-00018), a value > 0 was parameterised for the axis parameter P-AXIS-00472. The parameter P-AXIS-00472 cannot be used with spindles because spindles cannot be moved at rapid traverse.
Response | Class | 1 | Warning output, P-AXIS-00472 is set to zero.
Solution | Class | 1 | Assign P-AXIS-00472 a value of <= 0.
Parameter | %1: | Logical axis number [-]
%2: | Current value [-]
Parameterised value of P-AXIS-00018.
%3: | Incorrect value [-]
Parameterised value of P-AXIS-00472.
%4: | Corrected value [-]
Corrected value of P-AXIS-00472.
Error type | 2, Error message on data transfer of parameter lists to controller.