# Path length of relevant blocks (P-CHAN-00124)

P-CHAN-00124 | Path length of relevant blocks (B Spline)
Description | This parameter defines the maximum path length of relevant blocks. If blocks are longer than the specified length, the B Spline is deselected implicitly.
Parameter | hsc.bspline.max_path_length
Data type | REAL64
Data range | 0 ... MAX(REAL64)
Dimension | 0.1µm
Default value | 0
Remarks |