# ID 130134

New SIGNAL/WAIT-event could not be saved.
Description | Too many #SIGNAL or #WAIT have been used, and have not yet been acknowledged. The available controller memory is full. Depending on the configuration, 50 or 100 open signals and wait are permitted, see @@[SYSP].
Response | Class | 3 |
Solution | Class | 7 | Modify the CNC program and use less synchronization events. Deleting synchronizations that are no longer required .
Parameter | %1: | Current value [-]
Error type | 3, Error message from communication.