# ID 21987

Feed factor is out of permissible value range.
Description | An external path feed can be commanded via the PLC. In the NC program, this can be additionally weighted by a feed factor with #FF in [%] . The programmed feed factor here exceeds the permissible value range.
Response | Class | 2 | Abort NC program processing.
Solution | Class | 7 | Check and modify NC program. Program a feed factor within the permissible data range.
Parameter | %1: | Error value [%]
%2: | Lower limit value [%]
%3 | Upper limit value [%]
%4 |
%5 |
Error type | 1, Error message from NC program.