# ID 22194

Message to receiver via #MSG command is configured as warning.
Description | The channel parameters (P-CHAN-00518, P-CHAN-00519, P-CHAN-00520) can configure the behaviour of messages to each of the receivers via the #MSG command.. When this message occurs, the messages to the receiver are disabled in parameter 1 and are indicated as a warning.
Response | Class | 1 | No reaction
Solution | Class | 1 | Possible solutions are:

- Change channel parameter
- Delete the #MSG command

Parameter | %1: | Current value [-]
Current receiver of the #MSG command.
Error type | 1, Error message from NC program.