# Deselecting spline at exact stop G60 (P-CHAN-00421)

P-CHAN-00421 | Deselecting spline at programmed exact stop G60 (B Spline)
Description | This parameter defines the automatic deselection of B Spline interpolation for programmed exact stop G60 or G360.
Parameter | hsc.bspline.auto_off_g60
Data type | BOOLEAN
Data range | 0: No implicit deselection due to exact stop 1: Implicit deselection with programmed exact stop
Dimension | ----
Default value | 0
Remarks |