# ID 21044

DIN-syntax or programming only for main spindle.
Description | The DIN syntax is only permitted for the main spindle. The spindle used is not the main spindle [PROG//Section: Spindle programming].
Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Modify the NC program. 1st possibility : Change the main spindle with #MAIN SPINDLE 2nd possibility: Use spindle-specific syntax for the spindle to be programmed.
Parameter | %1: | Logical axis number [-]
Logical axis number of the programmed spindle
%2: | Logical axis number [-]
Logical axis number of the main spindle
Error type | 1, Error message from NC program.