# ID 110504

Changing the id of axis-specific current values transformation requires restart of the control.
Description | An attempt was made to change the transformation id of the actual value transformation P-AXIS-00381 by updating the axis parameter list. This is not possible; a change requires a controller restart.
Response | Class | 0 | Warning output, the value of P-AXIS-00381 is not changed.
Solution | Class | 0 | Change parameter and restart controller.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of axis
%2: | Current value [-]
Changed value of P-AXIS-00381
%3: | Corrected value [-]
Old value of P-AXIS-00381
Error type | 2, Error message on data transfer of parameter lists to controller.