# ID 150089

Number of inching keys does not match with number of logical inching keys.
Description | When interpreting manual mode parameters, the system detects that there are fewer handwheel parameter records than specified in parameter P-MANU-00008.
Response | Class | 3 | Manual mode parameters are not adopted in the CNC, but the CNC start-up is continued using default parameters.
Solution | Class | 6 | Correct value for parameter P-MANU-00008 or Add missing key parameter data records.
Parameter | %1: | Current value [-]
Value of parameter P-MANU-00008 in manual mode parameter data record.
%2: | Expected value [-]
Key parameter records were found during interpretation of manual mode parameters.
Error type | 2, Error message on data transfer of parameter lists to controller.