# ID 13163

Tool radius too large.
Description | A check is made as to whether the tool diameter of the current milling cutter taking into account the finishing allowance is less than the programmed width or length of the pocket. This message is displayed if the result is a violation of the pocket contour.
Response | Class | - | Error: Transition to error state. Complete reset of the NC channel necessary.
Solution | Class | - | Use a tool with a smaller diameter for machining so that the pocket contour is not violated.
Error type | 1, Error message from NC program.