# ID 13381

Distance between positions is not defined.
Description | The distance of a point in the first (@P4) or second (@P5) main direction is not defined or defined wrong. This is not permitted.
Response | Class | - | Error: Transition to error state. Complete reset of the NC channel necessary.
Solution | Class | - | Check parameter setting and correct input parameters @P4 and @P5.
Error type | 1, Error message from NC program.