# ID 120285

Axis exchange not permitted during active spline interpolation.
Description | No axis exchanges are permitted while Akima or B spline interpolation is active. For more information on spline function, see [PROG// Section: Akima spline interpolation] .[PROG// Section: B spline interpolation].
Response | Class | 2 | Program abort.
Solution | Class | 6 | Deactivate the spline function before releasing or requesting axes in the CNC program.
Error type | 1, Error message from NC program.