# ID 11016

Same object ID already in use.
Description | One cause of error can be the generation of communication objects of V.E. variables with great arrays. Extract from the V.E. List containing error that occurred # var[3].name VARIABLE_4 var[3].type REAL64

var[3].scope GLOBAL

var[3].synchronisation TRUE

var[3].array_size 3000

var[3].access_rights READ_WRITE

Error case

var[3].create_hmi_interface TRUE

Correction

var[3].create_hmi_interface FALSE

Alternatively, the number of communication objects declared in the V.E. list may be too big.

Response | Class | 3 | Abort job processing
Solution | Class | 7 | Reduce number of required communication objects
Parameter | %1: | Current value [-]
Concerning ID Nr.
%2: | Error value [-]
Name of the concerning object
%3: | Current value [-]
Name oft he object with the existing object ID
Error type | -