# ID 13125

Number of infeeds for thread cutting (@P11) is incorrect, must be a positive integer.
Description | Error in the definition of parameter @P11 for the machining mode. @P11 must be a positive integer.
Response | Class | - | Error: Transition to error state. Complete reset of the NC channel necessary.
Solution | Class | - | Check and correct the definition of infeed motions (@P11).
Error type | 1, Error message from NC program.