# ID 20133

Plane selection not allowed during active tool radius compensation.
Description | As long as the tool radius compensation is enabled, it is not permitted to program a plane selection via G17, G18 or G19. Example: Wrong: N10 G00 X0 Y0 Z0 N20 G41

N30 G19

N1000 M30

Correct:

N10 G00 X0 Y0 Z0

N20 G41

:

N25 G40

N30 G19

N35 G41

:

N999 G40

`N1000 M30`

Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify the NC program sequence. Deselect the TRC with G40 before programming plane selection.
Parameter | %1: | Error value [-]
Invalid G function
Error type | 1, Error message from NC program.