# ID 110035

Illegal numerator for damping value.
Description | The damping value for simulation drives is specified by numerator and denominator. Damping value = P-AXIS-00051 / P-AXIS-00050 An invalid value was specified for the numerator.
Response | Class | 1 | Warning and correction of parameter.
Solution | Class | 1 | Check and modify P-AXIS-00051 in the parameter list of the affected axis.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis
%2: | Error value [-]
Configured value of P-AXIS-00051
%3: | Limit value [-]
%4: | Corrected value [-]
P-AXIS-00051
Error type | 2, Error message by data transfer from parameter list into control device.